For 1990-2009 cars

### Removal Procedure

1. Remove the engine undercover shield. Refer to Engine Shield Replacement .
2. Drain the engine oil.
3. Remove the oil pan. Refer to Oil Pan Replacement .
4. Remove the oil strainer. Refer to Oil Pump Suction Pipe and Screen Assembly Replacement .
5. Remove the crankshaft balancer.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the crankshaft balancer.

Tighten
Tighten the crankshaft balancer bolts to 55 N·m (46 lb ft).

Important: Do not disassemble the crankshaft balancer. Otherwise, the engine and body may be able to vibrate.

2. Turn the crankshaft and align the crankshaft balancer 3-point on the gears.
3. Install the oil strainer. Refer to Oil Pump Suction Pipe and Screen Assembly Replacement .
4. Install the oil pan. Refer to Oil Pan Replacement .
5. Fill with engine oil.
6. Install the engine undercover shield. Refer to Engine Shield Replacement .