For 1990-2009 cars

#### Special Tools

J 21104-B (KM-475-B) Weatherstrip Remover Universal or equivalent

### Removal Procedure

1. Lower the rear window.
2. Pry off the inside door handle trim bezel.
3. Remove the power window control switch.
4. Disconnect the power window control switch electrical connector.
5. Remove the door trim panel screws.
6. Pry off the trim panel using the J 21104-B .

### Installation Procedure

1. Install the trim panel.
2. Connect the power window control switch electrical connector, if equipped.
3. Install the power window control switch.

Caution: Refer to Fastener Caution in the Preface section.

4. Install the door trim panel screws and tighten to 2.5 N·m (22 lb in).
5. Install the inside door handle trim bezel.
6. Raise the rear window.