For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the glove box, instrument panel lower cover, cigar lighter trim panel and stereo cassette player.
3. Remove the console cover.
4. Remove the screw from the rear portion of the floor console.
5. Remove the screws from the front portion of the floor console.
6. Remove the floor console.
7. Disconnect the electrical connectors.

### Installation Procedure

1. Connect the electrical connectors.
2. Install the floor console.
3. Install the front portion of the floor console with the screws.
4. Install the screws from the rear portion of the floor console.
5. Connect the negative battery cable.
6. Install the glove box, instrument panel lower cover, cigar lighter trim panel and stereo cassette player.
7. Install the console cover.