For 1990-2009 cars

### Removal Procedure

1. Remove the rotor. Refer to Front Brake Rotor Replacement.
2. Remove the bolts and the lockwashers for the splash shield from the steering knuckle.
3. Remove the splash shield.

### Installation Procedure

1. Install the splash shield.

Caution: Refer to Fastener Caution in the Preface section.

2. Secure the splash shield to the steering knuckle with the bolts and the lockwashers and tighten to 25 N·m (18 lb ft).
3. Install the rotor. Refer to Front Brake Rotor Replacement.