For 1990-2009 cars

Checks | Actions
--- | ---
Check the steering wheel for contact with the turn signal housing. | Adjust the turn signal housing.
Check the intermediate shaft joints for binding or looseness. | Replace the intermediate shaft.
Check the power steering pump flow control valve for sticking and improper alignment. | Replace the power steering pump.
Check the wheel alignment. | Align the wheels.
Check the wheel bearings for wear or damage. | Replace the wheel bearings.
Check the intermediate shaft joints for improper installation. | Adjust the intermediate shaft between the steering gear and the steering column. Replace the intermediate shaft.
Check the outer tie rods and the ball joints for binding or looseness. | Tighten the tie rods and the ball joints. Replace the tie rods and the ball joints.
Check the steering gear adjustments. | Perform a straight-ahead check.
Check the steering column shaft for rubbing on the shaft. | Replace the dash seal.
Check the steering shaft bearings for binding. | Replace the stub shaft bearings.
Check for binding in the ball joints. | Replace the ball joint.
Check for binding in the steering column. | Lubricate the steering column. Replace the steering column as needed.
Check the steering gear preload adjustment. | Perform a rack bearing preload adjustment.
Check for a sticking valve. | Lubricate the pinion valve assembly. Replace the pinion valve assembly, as needed.