For 1990-2009 cars

#### Special Tools

J 21104-B (KM-475-B) Weatherstrip Remover Universal or equivalent

### Removal Procedure

1. Lower the front window.
2. Remove the rear deck lid remote switch and the power window/mirror control switch.
3. Disconnect the electrical connectors.
4. Remove the door trim panel screws.
5. Pry off the trim panel using the J 21104-B .
6. Remove the door step lamp.

### Installation Procedure

1. Install the door step lamp.
2. Install the trim panel.
3. Connect the electrical connectors.
4. Install the rear deck lid remote switch and the power window/mirror control switch.

Caution: Refer to Fastener Caution in the Preface section.

5. Install the door trim panel screws and tighten to 2.5 N·m (22 lb in).
6. Raise the front window.