For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the left tire and wheel. Refer to Tire and Wheel Removal and Installation.
3. Using a suitable jack stand, support the rear of the powertrain.
4. Remove the transmission mount to bracket through bolt (1).
5. Remove the transaxle brace bolts (1, 3).
6. Remove the transaxle brace (2).
7. Remove the transmission mount to transmission bolts (2).
8. Remove the transmission mount (1).

### Installation Procedure

1. Install the transmission mount (1).

Caution: Refer to Fastener Caution in the Preface section.

2. Install the transmission mount to transmission bolts (2) and tighten to 90 N·m (66 lb ft).
3. Install the transaxle brace (2).
4. Install the transaxle brace bolt (1) and tighten to 50 N·m (37 lb ft).
5. Install the transaxle brace bolt (3) and tighten to 100 N·m (74 lb ft).
6. Install the transmission mount to bracket through bolt (1) and tighten to 90 N·m (66 lb ft).
7. Remove the jack stand.
8. Install the left tire and wheel. Refer to Tire and Wheel Removal and Installation.
9. Lower the vehicle.