For 1990-2009 cars

### Removal Procedure

1. Remove the control valve body assembly. Refer to Control Valve Body Replacement.
2. Remove the output speed sensor bolt and the sensor.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the output speed sensor and the bolt and tighten to 12 N·m (106 lb in)..
2. Install the control valve body assembly. Refer to Control Valve Body Replacement.