For 1990-2009 cars

#### Special Tools

DW-110-060 Engine Support Fixture

### Removal Procedure

1. Remove the air filter housing.
2. Install the DW-110-060 .
3. Support the transaxle with a supporting jack.
4. Remove the left 4 transaxle mounting bracket bolts.
5. Remove the transaxle mounting bracket cage bolt and nut.
6. Remove the left transaxle mounting bracket.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the left transaxle mounting bracket and 4 transaxle mounting bracket bolts and tighten to 40 N·m (30 lb ft).
2. Install the transaxle mounting bracket cage bolt and nut and tighten to 65 N·m (48 lb ft).
3. Remove the DW-110-060 .
4. Install the air filter housing.