For 1990-2009 cars

### Removal Procedure

1. Remove the caliper mounting bracket.
2. Remove the rotor detent screw.
3. Remove the rotor.
4. Remove the ABS sensor.
5. Remove the hub bolts and hub.
6. Remove the upper return spring, lower return spring and adjuster assembly.
7. Remove the retaining spring plate, spring and retaining spring pin.
8. Remove the parking brake shoe.
9. Remove the parking brake cable pin and cable from the backing plate.

### Installation Procedure

1. Install the parking brake cable to the backing plate and lock the pin.
2. Install the retaining spring pin, parking brake shoe, retaining spring and retaining spring plate.
3. Install the adjuster assembly, lower return spring and upper return spring.

Caution: Refer to Fastener Caution in the Preface section.

4. Install the hub with bolts and tighten to 65 N·m (48 lb ft).
5. Install the ABS sensor.
6. Install the rotor with detent screw and tighten to 4 N·m (35 lb in).
7. Install the caliper mounting bracket with bolts and tighten to 45 N·m (33 lb ft).
8. Install the wheel.