For 1990-2009 cars

### Front Panel

Points | Dimensions (mm) | Dimensions (in)
--- | --- | ---
Important: Reference dimensions show the distance between the center of positioning holes shown in illustrations.
A | 1,463 | 57.6
B | 1,094 | 43.1
C | 499 | 19.6
D | 648 | 25.5
E | 1,211 | 47.7
F | 1,345 | 53.0
G | 1,514 | 59.6
H | 1,298 | 51.1
I | 916 | 36.0
J | 1,106 | 43.5
K | 1,146 | 45.1

### Engine Compartment (1 of 3)

Points | Dimension (mm) | Dimension (in)
--- | --- | ---
Important: Reference dimensions show the distance between the center of positioning holes shown in illustrations.
A | 1,551 | 61.1
B | 1,471 | 58.0
C | 1,292 | 50.9
D | 1,232 | 48.5
E | 1,162 | 45.7
F | 1,041 | 41.0
G | 925 | 36.4
H | 1,232 | 48.5
I | 864 | 34.0
J | 1,028 | 40.5
K | 1,345 | 53.0
L | 1,441 | 56.7
M | 1,463 | 57.6
N | 1,470 | 57.9

### Engine Compartment (2 of 3)

Points | Dimension (mm) | Dimension (in)
--- | --- | ---
Important: Reference dimensions show the distance between the center of positioning holes shown in illustrations.
A | 899 | 35.4
B | 1,159 | 45.6
C | 923 | 36.3
D | 956 | 37.6
E | 1,696 | 66.8
F | 1,154 | 45.4
G | 740 | 29.1

### Engine Compartment (3 of 3)

Points | Dimension (mm) | Dimension (in)
--- | --- | ---
Important: Reference dimensions show the distance between the center of positioning holes shown in illustrations.
A | 538 | 21.2
B | 760 | 29.9
C | 1,635 | 64.4
D | 1,361 | 53.6
E | 830 | 32.7

### Back Panel Lower

Points | Dimension (mm) | Dimension (in)
--- | --- | ---
Important: Reference dimensions show the distance between the center of positioning holes shown in illustrations.
A | 1,083 | 42.6
B | 1,390 | 54.7
C | 1,039 | 41.0
D | 536 | 21.1
E | 896 | 35.3
F | 1,418 | 55.9

### Side Outer

Points | Dimension (mm) | Dimension (in)
--- | --- | ---
Important: Reference dimensions show the distance between the center of positioning holes shown in illustrations.
A | 375 | 14.8
B | 1,044 | 41.1
C | 1,098 | 43.2
D | 1,117 | 44.0
E | 1,018 | 40.1
F | 1,243 | 49.0
G | 1,058 | 41.7
H | 753 | 29.6
I | 553 | 21.8
J | 1,034 | 40.7

### Windshield and Rear Glass

Points | Dimension (mm) | Dimension (in)
--- | --- | ---
Important: Reference dimensions show the distance between the center of positioning holes shown in illustrations.
A | 1,354 | 53.3
B | 1,468 | 57.8
C | 1,457 | 57.7
D | 698 | 27.5
E | 1,093 | 43.0
F | 1,045 | 41.1
G | 1,337 | 52.6
H | 682 | 26.9
I | 1,265 | 50.0
J | 1,251 | 49.3

### Gap Chart - Front/Rear

Description | Location | Gap | Description | Location | Gap
--- | --- | --- | --- | --- | ---
Radiator Grille - Bumper | A | 5.0 + 2.0, 0 mm (0.19 + 0.08 in) | Trunk Lid - Bumper | R | 5.0 + 2.0, 0 mm (0.19 + 0.08 in)
Engine Hood - Radiator Grille | B | -- | Trunk Lid - Tail lamp | S | 3.8 + 1.0, 0 mm (0.15 + 0.039 in)
Engine Hood - Bumper | C | 5.0 +2.0, 0 mm (0.19 + 0.08 in) | Side Outer - Trunk Lid | T | 3.0 + 1.0, 0 mm (0.118 + 0.039 in)
Engine Hood - Headlamp | D | 4.5 + 1.0, -0.5 mm (0.18 + 0.039, 0.019 in) | Side Outer - Taillamp | U | 2.5 + 1.0, 0 mm (0.098 + 0.039 in)
Headlamp - Bumper | E | 3.5 ± 1.0 mm (0.14 ± 0.039 in) | Tail lamp - Bumper | V | 2.0 ± 1.0 mm (0.08 ± 0.039 in
Fender - Headlamp | F | 3.5 ± 1.0 mm (0.14 ± (0.039 in) | Side Outer - Bumper | W | 0 mm (0 in)
Fender - Bumper | G | 0 mm (0 in) | Trunk Lid - Rear Garnish | X | 1.5 ± 0.5 mm (0.06 ± 0.019 in)
Fender - Engine Hood | H | 3.0 + 0.1, -0.5 mm (0.118 + 0.039, 0.019 in) | -- | -- | --

### Gap Chart - Side

Description | Location | Gap | Description | Location | Gap
--- | --- | --- | --- | --- | ---
Front Pillar - Fender | I | 3.0 + 1.0, -0.5 mm ( 0.118 + 0.039, 0.019 in) | Side Outer - Rear Door | N | 3.5 + 1.0 mm (0.148 + 0.039 in)
Fender - Locker Panel | J | 5.0 ± 1 mm (0.200 ± 0.039 in) | Side Outer - Fixed Glass | O | 4.6 ± 1 mm (0.18 ± 0.039 in)
Front Door - Fender | K | 3.0 + 1.0, 0.5 mm (0.118 + 0.019 in) | Door - Locker Panel | P | 5.0 ± 1 mm (0.190-0.039 in)
Side Outer - Door | L | 4.6 ± 1 mm (0.18 ± 0.039 in) | Side Outer - Fuel Pillar Door | Q | 4.0 ± 0.3 mm (0.16 ± 0.11 in)
Front Door - Rear Door | M | 4.0 + 1.0, 0 mm (0.16 + 0.039 in) | - | - | -