For 1990-2009 cars

Connector 1: | JX203
Connector 2: | JX301
Connector 3: | JX302

### JX203

#### Connector Part Information

- OEM: ASIA 808613/831225/808121
- Service: N/A
- Description: 20-Way

#### JX203

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | BK | 250 | Ground
2 | D-GN | 44 | I/P Illumination Ground
3 | D-GN | 44 | I/P Illumination Ground
4 | D-GN | 44 | I/P Illumination Ground
5 | D-GN | 44 | I/P Illumination Ground
6 | D-GN | 44 | I/P Illumination Ground
7 | D-GN | 44 | I/P Illumination Ground (M98)
8 | D-GN | 44 | I/P Illumination Ground (M98)
9 | -- | -- | Not Used
10 | D-GN | 44 | I/P Illumination Ground
11 | BN/WH | 309 | I/P Illumination Power
12 | BN/WH | 309 | I/P Illumination Power
13 | BN/WH | 309 | I/P Illumination Power
14 | BN/WH | 309 | I/P Illumination Power
BN/WH | 309 | I/P Illumination Power
15 | BN/WH | 309 | I/P Illumination Power
16 | BN/WH | 309 | I/P Illumination Power
17 | BN/WH | 309 | I/P Illumination Power
18 | BN/WH | 309 | I/P Illumination Power (M98)
BN/WH | 309 | I/P Illumination Power (M98/MH7/MH8)
19 | BN/WH | 309 | I/P Illumination Power
20 | BN/WH | 309 | I/P Illumination Power

### JX301

#### Connector Part Information

- OEM: ASIA 808613/831225/808616
- Service: N/A
- Description: 20-Way F

#### JX301

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | L-BU | 14 | Turn Signal Switch - Left
2 | L-BU | 14 | Turn Signal Switch - Left
3 | L-BU | 14 | Turn Signal Switch - Left
4 | L-BU | 14 | Turn Signal Switch - Left
5 | L-BU | 14 | Turn Signal Switch - Left
6 | D-BU | 15 | Turn Signal Switch - Right
7 | D-BU | 15 | Turn Signal Switch - Right
8 | D-BU | 15 | Turn Signal Switch - Right
9 | D-BU | 15 | Turn Signal Switch - Right
10 | D-BU | 15 | Turn Signal Switch - Right
11 | BN/WH | 96 | Wiper Return
12 | BN/WH | 96 | Wiper Return
13 | BN/WH | 96 | Wiper Return
14 | L-BU | 20 | Stop Lamp Switch Signal
15 | L-BU | 20 | Stop Lamp Switch Signal
16 | L-BU | 20 | Stop Lamp Switch Signal
17 | L-BU | 20 | Stop Lamp Switch Signal
18 | L-BU | 263 | Tamper Switch Signal
L-BU | 263 | Tamper Switch Signal (Except Holden)
19 | L-BU | 263 | Tamper Switch Signal
20 | L-BU | 263 | Tamper Switch Signal

### JX302

#### Connector Part Information

- OEM: ASIA 808613/831225/808615
- Service: N/A
- Description: 20-Way F

#### JX302

Pin | Wire | Circuit | Function
--- | --- | --- | ---
1 | PK | 839 | Ignition 1 Voltage (- Holden)
L-BU | 14 | Left Turn Signal Lamp Supply Voltage (LLW)
2 | L-BU | 14 | Left Turn Signal Lamp Supply Voltage (LLW)
3 | PK | 839 | Ignition 1 Voltage (- Holden)
L-BU | 14 | Left Turn Signal Lamp Supply Voltage (LLW)
4 | PK | 839 | Ignition 1 Voltage (- Holden)
L-BU | 14 | Left Turn Signal Lamp Supply Voltage (LLW)
5 | PK | 839 | Ignition 1 Voltage (- Holden)
L-BU | 14 | Left Turn Signal Lamp Supply Voltage (LLW)
6 | L-GN | 24 | Backup Lamp Switch Signal
D-BU | 15 | Right Turn Signal Lamp Supply Voltage (LLW)
7 | L-GN | 24 | Backup Lamp Switch Signal
D-BU | 15 | Right Turn Signal Lamp Supply Voltage (LLW)
8 | L-GN | 24 | Backup Lamp Switch Signal
D-BU | 15 | Right Turn Signal Lamp Supply Voltage (LLW)
9 | L-GN | 24 | Backup Lamp Switch Signal (MFB/MFN)
D-BU | 15 | Right Turn Signal Lamp Supply Voltage (LLW)
10 | L-GN | 24 | Backup Lamp Switch Signal
D-BU | 15 | Right Turn Signal Lamp Supply Voltage (LLW)
11 | L-BU | 20 | Stop Lamp Supply Voltage (LLW)
12 | L-BU | 20 | Stop Lamp Supply Voltage (LLW)
13 | L-BU | 20 | Stop Lamp Supply Voltage (LLW)
14 | L-BU | 20 | Stop Lamp Supply Voltage (LLW)
15 | L-BU | 20 | Stop Lamp Supply Voltage (LLW)
16 | GY | 241 | Ignition 3 Voltage (C37/C38-LLW)
L-GN | 24 | Backup Lamp Switch Signal (LLW)
17 | GY | 241 | Ignition 3 Voltage (C37/C38-LLW)
L-GN | 24 | Backup Lamp Switch Signal (LLW)
18 | GY | 241 | Ignition 3 Voltage
L-GN | 24 | Backup Lamp Switch Signal (LLW)
19 | L-GN | 24 | Backup Lamp Switch Signal (LLW)
20 | L-GN | 24 | Backup Lamp Switch Signal (LLW)