For 1990-2009 cars

### Removal Procedure

1. Remove the front seat from the vehicle. Refer to Front Seat Cushion Replacement.
2. Remove the seat trims.
3. Remove the seat cushion bolts.
4. Remove the cushion from the seat track.

### Installation Procedure

1. Install the cushion onto the seat track.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the seat cushion with the bolts and tighten to 12 N·m (106 lb in).
3. Install the seat trims.
4. Install the front seat in the vehicle. Refer to Front Seat Replacement - Bucket.