For 1990-2009 cars

#### No Response to Movement of Shift Lever

Condition | Action
--- | ---
DEFINITION: No response to movement of shift lever
Gear Selector Assembly | Gear selector assembly mechanically broken or not connected to cable assembly
Gear Selector Cable |

• | Cable not connected to the gear selector assembly or to the manual shift shaft and detent lever assembly (710)

• | Cable broken internally

Manual Shift Shaft and Detent Lever Assembly (710) |

• | Not installed

• | Shaft broken

Manual Shift Shaft and Detent Lever Spring and Roller Assembly (711) |

• | Not installed

• | Mechanically broken, or mounting bolts (712, 715) not installed or loose

Manual Valve Link (336) |

• | Not installed

• | Not connected to the manual shift shaft assembly (710)