For 1990-2009 cars

Checks | Actions
--- | ---
Check for an out-of-balance tire or wheel. | Balance the tire or the wheel.
Check for excessive wheel hub runout. |

• | Measure the hub flange runout.

• | Replace the hub, as needed.

Check for excessive brake drum or brake rotor imbalance. |

• | Adjust the brakes.

• | Replace the brake rotor or the brake drum, as needed.

Check for worn tie rod ends. | Replace the outer tie rods.
Check for wheel trim imbalance. | Balance the wheel.
Check for a worn lower ball joint. | Replace the lower ball joint.
Check for excessive wheel runout. |

• | Measure the wheel runout.

• | Replace the wheel, as needed.

Check for excessive loaded radial runout on the tire and the wheel assembly. | Match-mount the tire and the wheel assembly.