For 1990-2009 cars

### Removal Procedure

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .
2. Remove the console. Refer to Front Floor Console Replacement .
3. Remove the shift control cable adjust locks (1).
4. Remove the shift control cables (2) from the shift control lever housing bracket.
5. Disconnect the shift control cables from the shift control adjusters.
6. Remove the shift control cables (1) from the transaxle using a suitable tool.
7. Remove the cables (2) from the shift control cable bracket.
8. Remove the grommet from the dash panel.
9. Remove the shift control cables from the vehicle.

### Installation Procedure

1. Install the shift control cables to the vehicle.
2. Install the grommet to the dash panel. Ensure that the shift control cable pass-through grommet is properly seated and the grommet arrow is pointing up.
3. Install the cables (2) to the shift control cable bracket.
4. Install the shift control cables (1) to the transaxle.
5. Position the transaxle into NEUTRAL.
6. Connect the shift control cables into the shift control adjusters.
7. Install the shift control cables to the shift control lever housing bracket.
8. Position the shift lever into NEUTRAL.
9. With the shift cable ends in the adjusters, adjust the cables by pushing the neutral lock pin. Move the shifter slightly to center the neutral lock pin.
10. Press and lock the shift control cable adjust locks.
11. Pull the neutral lock pin to the original position.
12. Install the console. Refer to Front Floor Console Replacement .
13. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .