For 1990-2009 cars

### Removal Procedure

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the rear stabilizer link. Refer to Stabilizer Shaft Link Replacement .
3. Remove the rear stabilizer bar bolt, U-clamp, and bushing.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the rear stabilizer bar bolt, U-clamp, and bushing.

Tighten
Tighten the rear stabilizer bar bolt to 50 N·m (37 lb ft).

2. Install the rear stabilizer link. Refer to Stabilizer Shaft Link Replacement .