For 1990-2009 cars

## Clutch Noisy D33 Manual Transaxle

Checks | Actions
--- | ---
Check for insufficient lubrication of clutch pedal bushing. | Lubricate the clutch pedal brushing
Check for interference of clutch pedal return spring. | Remove and reinstall the clutch pedal return spring.

## Clutch Noisy D24 Manual Transaxle

Checks | Actions
--- | ---
Check for a worn release bearing. | Replace the worn release bearing.
Check for an improperly installed release lever. | Remove and properly reinstall the fork shaft. Very lightly lubricate the fork fingers at the release bearing with wheel bearing grease.