For 1990-2009 cars

### Removal Procedure

1. Reposition the plastic caps to reveal the assist handle screws.
2. Remove the screws and the assist handle from the headliner.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the assist handle to the headliner with the screws.

Tighten
Tighten the passenger assist handle screws to 3 N·m (27 lb in).

2. Install the plastic caps over the assist handle screws.