For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the console cover.
3. Remove the screws and the ashtray housing.
4. Remove the bulb from the ashtray lamp housing.
5. Disconnect the bulb from the ashtray lamp housing electrical connector.

### Installation Procedure

1. Connect the replacement bulb to the ashtray lamp housing electrical connector.
2. Install the replacement bulb into the ashtray lamp housing.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the ashtray housing with the screws.

Tighten
Tighten the ashtray housing screws to 2.5 N·m (22 lb in).

4. Install the console cover.
5. Connect the negative battery cable.