For 1990-2009 cars

### Removal Procedure

1. Raise and suitable support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the stabilizer shaft-to-stabilizer link nut.
3. Remove the stabilizer link-to-control arm nut.
4. Remove the stabilizer link.

### Installation Procedure

Note: The weight of the vehicle must be supported by the control arms before the stabilizer link-to-control arm nuts or the stabilizer shaft-to-stabilizer link nuts are tightened. This can be done by lowering the vehicle onto jackstands under the control arms.

1. Lower the vehicle so the control arms are supported by jackstands.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the stabilizer link and nuts and tighten to 50 N·m (37 lb ft).