For 1990-2009 cars

### Removal Procedure

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the rear wheels.
3. Remove the rear muffler. Refer to Exhaust Muffler Replacement.

Warning: Failure to support crossmember can cause crossmember to drop to the ground when crossmember mounting bolts are removed.

4. Remove the rear seat and rear strut upper nut-to-body.
5. Remove the rear crossmember bolts and nuts.
6. Remove the rear crossmember by lowering the jackstand.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the rear crossmember with bolts and nuts.

Tighten
Tighten the rear crossmember bolts and nuts to 110 N·m (81 lb ft).

2. Install the front/rear parallel links and stabilizer bar.