For 1990-2009 cars

#### Special Tools

DW-110-060 Engine Assembly Support Fixture

### Removal Procedure

1. Remove the engine cover. Refer to Engine Cover Replacement .
2. Remove the surge tank. Refer to Radiator Surge Tank Replacement .

Important: Only lift the engine far enough to take the weight off the engine mount assembly, or damage to the mount and lifting equipment failure may occur.

3. Support the engine assembly using DW-110-060 .
4. Remove the engine mount adapter retaining bolts from the engine mount support bracket.
5. Remove the engine mount frame side bracket retaining bolt and nuts.
6. Remove the engine mount assembly.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the engine mount assembly.

Tighten

• | Tighten the engine mount bracket retaining bolt to 65 N·m (47.9 lb ft).

• | Tighten the engine mount assembly nuts to 90 N·m (66.4 lb ft).

• | Tighten the engine mount retaining bolts and nuts to 50 N·m (37 lb ft).

2. Remove the DW-110-060 .
3. Install the surge tank. Refer to Radiator Surge Tank Replacement .
4. Install the engine cover. Refer to Engine Cover Replacement .