For 1990-2009 cars

### Removal Procedure

1. Reposition the weatherstrip in order to access the screws.
2. Remove the screws and the front door body side molding, shown, rear door rear quarter upper trim panel molding similar.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the screws and the front door body side, shown, rear door rear quarter upper trim panel molding similar.

Tighten
Tighten the front door body side molding screws to 1.3 N·m (12 lb in).

2. Install the weatherstrip to its original position.