For 1990-2009 cars

### Removal Procedure

1. Disconnect the speedometer driven gear electrical wiring connector.
2. Remove the speedometer driven gear bolt.
3. Remove the speedometer driven gear.

### Installation Procedure

1. Install the speedometer driven gear.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the speedometer driven gear bolt.

Tighten
Tighten the speedometer driven gear bolt to 3-5 N·m (27-44 lb in).

3. Connect the speedometer driven gear electrical wiring connector.