For 1990-2009 cars

#### Tools Required

• | J 23327 Clutch Spring Compressor

• | J 23456 Booster and Clutch Pack Compressor

• | J 45184 Differential Bearing Race Installer

Important: Do not damage the 1-2 reverse clutch piston seals (602, 603).

1. Apply automatic transmission fluid to the new 1-2 reverse clutch piston seals (602, 603).
2. Install the new 1-2 reverse clutch piston inner seal (602) and the 1-2 reverse clutch piston outer seal (604) onto the 1-2 reverse clutch piston (603).
3. Apply automatic transmission fluid to the inner surface of the transmission case cover.
4. Hand press the 1-2 reverse clutch piston (603) into the transmission case cover, making sure not to damage the seals.

Important: Do not bend the 1-2 reverse clutch piston return spring assembly (601).

5. Place the 1-2 reverse clutch piston return spring assembly (601) on the 1-2 reverse clutch piston (603), indexing the springs into the holes in the 1-2 reverse clutch piston assembly.
6. Place J 45184 (1) on the center of J 23456 (2).
7. Place the transmission case cover (19) with the 1-2 reverse clutch piston assembly onto J 45184 (1).
8. Using J 23327-1 (3), which is the bridge part of J 23327 , compress the 1-2 reverse clutch piston return spring assembly (601).
9. Install the 1-2 reverse clutch piston return spring retaining ring (600) using snap ring pliers.
10. Remove the pressure from J 23456 (2).
11. Remove all tools.

Important: Check the position and direction of the 1-2 reverse clutch apply plate (618) before installation.

12. Install the 1-2 reverse clutch apply plate (618).

Important:

• | Make sure you have the correct number of clutch plates.

• | Make sure the clutch plates are in the correct order.

13. Install the 6 steel plates (619) and the 6 fiber plates (620).
14. Install the 1-2 reverse clutch backing plate (621).

Important: Check the position of the 1-2 reverse clutch backing plate retaining ring (622) before installation.

15. Install the 1-2 reverse clutch backing plate retaining ring (622) into the groove indicated.