For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Remove the battery negative cable.
2. Remove the radiator grill upper cover.
3. Remove the radiator grill lower cover.
4. Disconnect the auxiliary cooling fan connector.
5. Remove the auxiliary cooling fan retaining bolts.
6. Remove the auxiliary cooling fan downward.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

Warning: To help avoid personal injury or damage to the vehicle, a bent, cracked, or damaged fan blade or housing should always be replaced.

1. Install the auxiliary cooling fan using the retaining bolts and tighten to 4 N·m (35 lb in).
2. Install the radiator grill upper and lower covers.
3. Connect the battery negative cable.