For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Disconnect the ignition coil wiring harness connectors.
3. Remove the ignition coils.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the ignition coils using the ignition coil retaining bolts and tighten to 7 N·m (62 lb in).
2. Connect the ignition coil wiring harness connectors.
3. Connect the negative battery cable.