For 1990-2009 cars

#### Special Tools

J 36346 Fascia Retainer Remover

### Removal Procedure

1. Remove the battery tray. Refer to Battery Tray Replacement.
2. Using the J 36346 , disconnect the shift control cable from the transaxle range switch lever.
3. Remove the transaxle range switch lever nut and lever.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the transaxle range switch lever and lever nut and tighten to 16 N·m (12 lb ft).
2. Install the shift control cable end fitting onto the ball stud of the transaxle range switch lever. An audible snap will be heard when properly installed.
3. Install the battery tray. Refer to Battery Tray Replacement.