For 1990-2009 cars

### Removal Procedure

1. Remove the rear bumper fascia. Refer to Rear Bumper Fascia Replacement.
2. Remove the rear bumper energy absorber, if equipped. Refer to Rear Energy Absorber Replacement.

Note: The 5 mph (8 km/h) bumper assembly is shown. The 2.5 mph (4km/h) bumper assembly similar.

3. Remove the nuts and the impact bar.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the impact bar with the nuts and tighten to 9 N·m (80 lb in).
2. Install the rear bumper energy absorber, if equipped. Refer to Rear Energy Absorber Replacement.

Note: The 5 mph (8 km/h) bumper assembly is shown. The 2.5 mph (4km/h) bumper assembly similar.

3. Install the rear bumper fascia. Refer to Rear Bumper Fascia Replacement.