For 1990-2009 cars

### Removal Procedure

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Place a drain pan or suitable container under the vehicle.
3. Remove the inlet pipe union bolt from the radiator.
4. Remove the outlet pipe union bolt and the clip bolt from the radiator.
5. Remove the oil cooler line assembly bolt from the transaxle.
6. Remove the oil cooler line assembly.
7. Replace the transaxle oil cooler line seals. Refer to Transmission Fluid Cooler Pipe Seal Replacement .

### Installation Procedure

1. Install the oil cooler line assembly to the transaxle.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the oil cooler line assembly bolt.

Tighten
Tighten the oil cooler line assembly bolt to 10 N·m (89 lb in).

3. Install the outlet pipe union bolt and the clip bolt to the radiator.

Tighten

• | Tighten the outlet pipe union bolt (1) to 33 N·m (24 lb ft).

• | Tighten the clip bolt (2) to 9 N·m (80 lb in).

4. Install the inlet pipe union bolt to the radiator.

Tighten
Tighten the inlet pipe union bolt to 33 N·m (24 lb ft).

5. Lower the vehicle.
6. Add fluid to the transaxle.
7. Check the fluid level. Refer to Transmission Fluid Replacement .