For 1990-2009 cars

Table 1: | Fluid Pump w/Valve Trains Assemble
Table 2: | Torque Converter Fluid Seal and Fluid Filter Assembly Assemble

### Fluid Pump w/Valve Trains Assemble

Callout | Component Name
--- | ---
1 | Fluid Pump Driven Gear Tip The chamfer on the driven gear O.D. faces the pump body.
2 | Fluid Pump Drive Gear Tip The chamfer on the drive gear teeth face towards the pump body.
3 | Fluid Pump Cover
4 | Fluid Pump Cover Bolts M6 x 25 (Qty: 23) Caution: Refer to Fastener Caution in the Preface section.

#### Tighten

12 N·m (106 lb in)

5 | TCC Control Valve Train
6 | Fluid Pump Blow Off Ball Valve Train
7 | Pressure Regulator Valve Train
8 | TCC Blow Off Ball Valve Train

### Torque Converter Fluid Seal and Fluid Filter Assembly Assemble

Callout | Component Name
--- | ---
1 | Torque Converter Fluid Seal Assembly Tip The fluid seal assembly must be staked in place using DT-47792-2 which is part of DT-47792 to ensure proper seal retention.

#### Special Tool

DT-47792 Seal Installer

2 | Torque Converter Fluid Seal

#### Special Tool

DT-47791 Seal Installer

3 | Torque Converter Fluid Seal Retainer
4 | Fluid Filter Assembly Tip Rotate filter 90 degrees to engage locking tangs.