For 1990-2009 cars

Callout | Component Name
--- | ---
1 | Control Solenoid Valve Assembly Filter Plate Notice: Use care when removing or installing the filter plate assembly. A broken or missing retaining tab may not adequately secure the filter plate to the control solenoid valve assembly, resulting in possible damage or contamination.

Tip
Install a NEW filter plate to prevent fluid leaks past the fluid seals.

2 | Control Solenoid (w/Body and TCM) Valve Assembly
3 | Control Valve Body Bolt M5 x 40.5 (Qty: 3) Notice: Refer to Fastener Notice in the Preface section. Tighten Tighten to 8 N·m (71 lb in).
4 | Control Valve Body Bolt M6 x 97 (Qty: 12) Tighten Tighten to 12 N·m (106 lb in).