For 1990-2009 cars

1. Install a new gasket (820) on the drain plug (819).

Caution: Refer to Fastener Caution in the Preface section.

2. Install the drain plug (819) into the case assembly (17) and tighten to 39 N·m (29 lb ft).
3. Install the vent hose assembly.
4. Install a new o-ring (824) on the transmission fluid level indicator and lubricate with transmission fluid.
5. Install the transmission fluid level indicator.
6. Install the transmission fluid level indicator bolt and tighten to 10 N·m (89 lb in).