For 1990-2009 cars

## Rocker Panel Molding Replacement Production Molding

### Removal Procedure

1. Remove the front mud guards. Refer to Rear Mud Flap Guard Replacement.
2. Remove the screws and the rocker panel molding.

### Installation Procedure

1. Install the rocker panel molding with the screws.
2. Instal the front mud guards. Refer to Rear Mud Flap Guard Replacement.

## Rocker Panel Molding Replacement Accessory Molding

### Removal Procedure

1. Remove the lower rocker molding clips.
2. Remove the rocker molding end clips.
3. Remove the screws.
4. Remove the rocker molding.

### Installation Procedure

1. Install the rocker panel molding.
2. Install the rocker molding end clips.
3. Install the rocker molding lower clips.

Notice: Refer to Fastener Notice in the Preface section.

4. Install the rocker panel molding screws.

Tighten
Tighten the rocker panel molding screws to 2 N·m (18 lb in)