For 1990-2009 cars

### Removal Procedure

1. Raise the vehicle.
2. Remove the drain plug and drain fluid. Allow at least 5 minutes for the fluid to drain completely.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the drain plug and tighten to 12 N·m (106 lb in).
2. Add the transmission fluid to the transaxle through the fill cap.
3. Perform the transmission fluid checking.