For 1990-2009 cars

#### Wire Color Chart

Wire Color | Abbreviation on Schematic
--- | ---
Dark Green | D-GN
Light Green | L-GN
Dark Blue | D-BU
Brown | BN
Orange | OG
Yellow | YE
Grey | GY
Light Blue | L-BU
Red | RD
Black | BK
Pink | PK
White | WH
Purple | PU

#### Wires with Tracers

Wire Color | Abbreviation on Schematic
--- | ---
Red with White Tracer | RD/WH
Red with Black Tracer | RD/BK
Brown with White Tracer | BN/WH
Black with White Tracer | BK/WH
Black with Yellow Tracer | BK/YE
Green with Black Tracer | D-GN/BK
Green with White Tracer | D-GN/WH
Light Green with Black Tracer | L-GN/BK
Red with Yellow Tracer | RD/YE
Red with Blue Tracer | RD/D-BU
Black with Brown Tracer | BK/BN

OLD Symbol | NEW Symbol | Description
--- | --- | ---
|  | Supplemental Inflatable Restraint (SIR) or Supplemental Restraint System (SRS) Icon This icon is used to alert the technician that the system contains SIR/SRS components that require certain precautions before servicing.
|  | Voltage Indicator Boxes These boxes are used on schematics to indicate when voltage is present at a fuse.
|  | Partial Component When a component is represented in a dashed box, the component or its wiring is not shown in its entirety.
|  | Entire Component When a component is represented in a solid box the component or its wiring is shown in its entirety.
|  | Fuse
|  | Connector Attached to Component
|  | Pigtail Connector
|  | Bolt On or Screw On Eyelet Terminal
|  | Inline Harness Connector
|  | Splice
|  | Chassis Ground
|  | Case Ground
|  | Single Filament Light Bulbs
|  | Light Emitting Diodes
|  | Battery
|  | Resistor
|  | Variable Resistor
|  | Position Sensor
|  | Diode
|  | Heating Element
|  | Motor
|  | Solenoid
|  | Coil
|  | Antenna
|  | Shield
|  | Switches
|  | Single Pole/Throw Relay - Normally Open
|  | Single Pole/Throw Relay - Normally Closed