For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the upper and the lower steering column cover panel by removing the screws.
3. Remove the audio system trim plate and audio to allow enough working space for the removal of instrument cluster trim panel screws. Refer to Radio Replacement.
4. Remove the instrument panel under cover. Refer to Front Floor Console Extension Replacement - Side.
5. Remove the knee bolster. Refer to Knee Bolster Replacement.
6. Remove the instrument cluster trim panel. Refer to Instrument Cluster Replacement.
7. Remove the steering column jacket assembly securing bolts and nuts.
8. Set the ignition key to ACC position.
9. Remove the key cylinder by pushing the disassemble button and pulling out the key, at the same time.

### Installation Procedure

1. Set the ignition key to the ACC position.
2. Install the key cylinder by pushing it into the key cylinder housing.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the steering column jacket assembly securing bolts and nuts and tighten to 22 N·m (16 lb ft).
4. Install the instrument cluster trim panel. Refer to Instrument Cluster Replacement.
5. Install the instrument panel under cover. Refer to Front Floor Console Extension Replacement - Side.
6. Install the knee bolster. Refer to Knee Bolster Replacement.
7. Install the audio system trim plate. Refer to Radio Replacement.
8. Install the upper and the lower steering column cover panel. Tighten the screws to 2.5 N·m (22 lb in).
9. Connect the negative battery cable.