For 1990-2009 cars

1. Inspect the components that are still on the transmission case for the following conditions:

• | Loose, cross-threaded, or damaged threads on the transmission oil cooler fittings

• | A loose, missing, or damaged transmisssion name plate

2. Inspect the transmission case for the following conditions:

• | Gasket sealing surfaces that are damaged or have porosity

• | Bolt and screw holes that are stripped or damaged - repair with thread insert

• | Damaged or porous case and fluid passages

• | Damaged snap ring grooves or housing splines

• | A loose, cross threaded, or damaged pressure test plug and fluid level hole plug