For 1990-2009 cars

### Removal Procedure

1. Using a suitable tool disengage the right hand side trim panel (2) retaining clips and remove the trim panel (2) from the I/P pad (1).
2. Using a suitable tool disengage the left hand side trim panel (3) retaining clips and remove the trim panel (3) from the I/P pad (1).

### Installation Procedure

1. Align the left hand trim panel (3) with the I/P pad (1).
2. Install the trim panel (3) by firmly engaging the retaining clips.
3. Align the right hand trim (2) panel with the I/P pad (1).
4. Install the trim panel (2) by firmly engaging the retaining clips.

### Removal Procedure - (SV6, SS and SSV)

1. Using a suitable tool disengage the trim panel (1) retaining clips.
2. Remove the trim panel (1) from the I/P pad.

### Installation Procedure

1. Align the trim panel (1) with the I/P pad.
2. Install the trim panel (1) to the I/P pad by engaging the retaining clips.
3. Ensure the trim panel (1) is flush with the I/P pad.