For 1990-2009 cars

### Removal Procedure

1. Remove the rear header trim. Refer to Roof Panel Rear Applique Replacement .
2. Remove the body lock pillar trim to body retaining screw (1).

Important: Pull the top of the body lock pillar trim (2) to disengage the retaining clip (1) and slide out the bottom of the body lock pillar trim (2) to disengage the retaining tangs (4).

3. Remove the body lock pillar trim (2) from the body (3).

### Installation Procedure

Important: Slide in the bottom of the body lock pillar trim (2) to engage the retaining tangs (4). Push in the top of the body lock pillar trim (2) to engage the retaining clip (1).

1. Install the body lock pillar trim (2) to the body (3).

Notice: Refer to Fastener Notice in the Preface section.

2. Install the body lock pillar trim to body retaining screw (1).

Tighten
Tighten the screw to 2 N·m (18 lb ft).

3. Install the rear header trim. Refer to Refer to Roof Panel Rear Applique Replacement .