For 1990-2009 cars

### Removal Procedure

1. Remove the front seat outer trim cover. Refer to Seat Cushion Outer Trim Panel Replacement.

Important: Carefully disengage the door sill plate (1), take care not to damage the door sill plate (1).

2. Remove the door sill plate (1) from the door sill (2).

### Installation Procedure

Important: Carefully engage the door sill plate (1), take care not to damage the door sill plate (1).

1. Install the door sill plate (1) to the door sill (2).
2. Install the front seat outer trim cover. Refer to Seat Cushion Outer Trim Panel Replacement.