For 1990-2009 cars

#### Tools Required

J 41712 Oil Pressure Sensor Socket

### Removal Procedure

1. Turn the ignition OFF.
2. Remove the left hand engine cover. Refer to Engine Cover Replacement.
3. Disconnect the oil pressure sensor electrical connector (1).

Important: A small amount of oil will drain out of the oil filter housing when the oil pressure sensor is removed. Use a shop towel to absorb the oil.

4. Use the J 41712 in order to remove the oil pressure sensor (1).

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Use the J 41712 in order to install the oil pressure sensor (1).

Tighten
Tighten the oil pressure sensor to 20 N·m (15 lb ft).

2. Connect the oil pressure sensor electrical connector (1).
3. Install the left hand engine cover. Refer to Engine Cover Replacement.