For 1990-2009 cars

## Temperature Valve Actuator Replacement - Right Side RHD

### Removal Procedure

1. Remove the right side console lower extension. Refer to Instrument Panel Extension Replacement.
2. Remove right side floor duct. Refer to Floor Air Outlet Duct Replacement - Right Side.
3. Disconnect the driver air mix actuator electrical connector (2).
4. Remove the driver air mix actuator to HVAC module assembly retaining screws (3).
5. Remove the driver air mix actuator from the HVAC module assembly (4).

### Installation Procedure

1. Align the actuator drive gear (1) with the door shaft spline (2).
2. Install the driver air mix actuator (1) to HVAC module assembly (4).

Notice: Refer to Fastener Notice in the Preface section.

3. Install the driver air mix actuator to HVAC module assembly retaining screws (3).

Tighten
Tighten the screws to 1 N·m (9 lb ft).

4. Connect the driver air mix actuator electrical connector (2).
5. Install the right side floor duct. Refer to Floor Air Outlet Duct Replacement - Right Side.
6. Install the right side console lower extension. Refer to Instrument Panel Extension Replacement.
7. Perform HVAC system relearn. Refer to HVAC Control Module Programming and Setup.