For 1990-2009 cars

## Temperature Valve Actuator Replacement - Left Side RHD

### Removal Procedure

1. Remove the I/P lower trim plate assembly. Refer to Instrument Panel Insulator Panel Replacement - Left Side.
2. Remove the I/P compartment assembly. Refer to Instrument Panel Compartment Replacement.
3. Remove left side floor duct. Refer to Floor Air Outlet Duct Replacement - Left Side.
4. Disconnect the passenger air mix mode actuator electrical connector (2).
5. Remove the passenger air mix mode actuator to HVAC module assembly retaining screws (3).
6. Remove the passenger air mix actuator (1) from the HVAC module assembly (4).

### Installation Procedure

1. Align the actuator drive gear (1) with the door shaft spline (2).
2. Install the passenger air mix actuator (1) to the HVAC module assembly (4).

Notice: Refer to Fastener Notice in the Preface section.

3. Install the passenger air mix actuator to HVAC module assembly retaining screws (3).

Tighten
Tighten the screws to 1 N·m (9 lb ft).

4. Connect the passenger air mix actuator electrical connector (2).
5. Install left side floor duct. Refer to Floor Air Outlet Duct Replacement - Left Side.
6. Install the I/P compartment assembly. Refer to Instrument Panel Compartment Replacement.
7. Install the I/P lower trim plate assembly. Refer to Instrument Panel Insulator Panel Replacement - Left Side.
8. Perform HVAC system relearn. Refer to HVAC Control Module Programming and Setup.