For 1990-2009 cars

Callout | Component Name
--- | ---
Notice: Refer to Fastener Notice in the Preface section. Fastener Tightening Specifications: Refer to Fastener Tightening Specifications .

#### Preliminary Procedures

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the transmission fluid pan and filter. Refer to Automatic Transmission Fluid, Fluid Pan and/or Filter Replacement .
3. Remove the transmission electrical connector. Refer to Automatic Transmission Electrical Connector Passage Sleeve Replacement .

1 | Manual Shaft Detent Bolt Tighten 12 N·m (106 lb. in)
2 | Manual Shaft Detent Assembly
3 | Control Valve Assembly Bolt (Qty: 6)

• | Do not remove all the bolts in the control valve body assembly. Remove only the bolts indicated.

• | Tighten in specified sequence.

Tighten
8 N·m (71 lb. in)

4 | Control Valve Assembly
5 | Fluid Pump Seal Discard seal and replace with new.
6 | Fluid Pump Seal Discard seal and replace with new.
7 | Centre Support Fluid Passage Seal Discard seal and replace with new.