For 1990-2009 cars

#### Electrical Information Reference

• | Diagnostic System Check - Vehicle.

• | Circuit Testing.

• | Testing for Intermittent Conditions and Poor Connections.

The alternator warning indicator is only illuminated for 6 seconds after the ignition is switched to the ON position with the engine OFF.

Caution: Refer to Safety Glasses Caution in the Preface section.

1. Carry out the Diagnostic System Check.
2. Ignition on alternator warning light should illuminate for 6 second.

⇒ | If the alternator warning does not illuminate, connect the scan tool and command the alternator warning light ON.

⇒ | If the light does not illuminate replace instrument panel cluster.

### Repair Instructions

Instrument Cluster Replacement.