For 1990-2009 cars

## Instrument Panel Insulator Panel Replacement - Left Side RHD

### Removal Procedure

1. Grasp the I/P lower trim plate assembly (1) and carefully pull downward to disengage the retaining clips.
2. Remove the courtesy lamp socket assembly (2) from the left lower trim plate by turning the socket counter-clockwise.
3. Remove the I/P lower trim plate assembly (1).

### Installation Procedure

1. Install the courtesy lamp socket assembly (2) to the I/P lower trim plate assembly (1).
2. Align the I/P lower trim plate assembly (1) to the I/P.
3. Attach the I/P lower trim plate assembly (1) to the I/P by engaging the retaining clips.
4. Ensure all clips are located correctly.