For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Rear Drive Shaft to Rear Hub Retaining Nut
There are two alternate methods of achieving the required Rear Hub Retaining Nut torque. Important: DO NOT EXCEED THE SPECIFIED TIGHTENING VALUES, otherwise premature bearing failure may result.
Preferred Method |  |

- First Pass

150 N·m

110 lb ft

- Loosen

-180 Degrees

- Final Pass

425 N·m

313 lb ft

Alternate Method

- First Pass

150 N·m

110 lb ft

- Loosen

-180 Degrees

- Second Pass

50 N·m

37 lb ft

- Final Pass

45 Degrees