For 1990-2009 cars

### Removal Procedure

1. Using a suitable flat blade tool, remove the centre console upper retaining screw cover (1) from the centre console end panel (2).
2. Remove the centre console end panel to centre console upper retaining screws (1).
3. Using a suitable flat blade tool, remove the centre console lower retaining screw cover (1) from the centre console end panel (2).
4. Remove the centre console end panel to centre console lower retaining screws (2).
5. Remove the centre console end panel (1) from the centre console (3).

### Installation Procedure

1. Install the centre console end panel (1) to the centre console (3).

Notice: Refer to Fastener Notice in the Preface section.

2. Install the centre console end panel to centre console lower retaining screws (2).

Tighten
Tighten the screws to 2 N·m (18 lb in).

Important: Listen for an audible click from the centre console lower retaining screw cover (1) to confirm fitting.

3. Install the centre console lower retaining screw cover (1) to the centre console end panel (2).
4. Install the centre console end panel to centre console upper retaining screws (1).

Tighten
Tighten the screws (1) to 2 N·m (18 lb in).

Important: Listen for an audible click from the centre console end panel retaining screw cover (1) to confirm fitting.

5. Install the centre console end panel retaining screw cover (1) to the centre console (2).